**FT\_DS-G10 E-L-V2.0.2.231219**



|  |  |
| --- | --- |
| Components |  LF 2 x 8 (Neodymium magnet) / HF 1 x 3 (75mm Neodymium magnet) |
| Connectors |  2 x NEUTRIK NL4 |
| Frequency response |  65Hz-18KHz |
| Sensitivity (1W/1M) |  101 dB |
| Maximum sound pressure |  127 dB |
| Rated power |  550 Watts |
| Maximum power |  1100 Watts |
| Nominal impedance |  8Ω |
| Coverage |  H 110°×V10° |
| Height x width x depth |  250 x 700 x 379mm |
| Weight |  23.5 Kg |

**Specification:**